# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: TENDER FOR THE** **SUPPLY AND DELIVERY OF FUEL FOR THE CONSTRUCTION OF WATER FOR LIVESTOCK PRODUCTION FACILITIES**

**p 1 /…**

**Reference:** **MOBIP/SUPLS/2.6/2.6.2/T3SF**

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

| **Item**  | **2. Specifications required** | **3. Specifications offered** | **4. Notes, remarks, ref to documentation** | **5. Evaluation committee’s notes**  |
| --- | --- | --- | --- | --- |
| **1** | Diesel AGO (AGO must have a density @ 20 degrees centigrade in Kg/m3 of between 820-870 and have Cetane index of 48 minimum and Sulphur content of 0.05% maximum.)   |  |  |  |
| **2** | Petrol PMS (PMS must have a density @ 20 degrees centigrade in Kg/m3 of between 716-771 and have Cetane index of 50 minimum and Sulphur content of 0.01% maximum.)  |  |  |  |

**Locations of Valley Tanks for Construction/Rehabilitation by MOBIP - delivery locations (Provision List)**

1. Luwero (Natyaaba VT. 20,000m3),
2. Mityana (Mpongo VT 20,000m3)
3. Nakasongola (KalungiVT 10,000m3),
4. Kiboga (Kateega VT 10,000m3).
5. Kiruhura (Rwendama VT 20,000m3),
6. Masaka (Kasange VT 20,000m3),
7. Kyotera (Kabano VT 20,000m3)
8. Mbarara (Nombe VT 10,000m3)
9. Kiryandongo (Kente VT 10,000m3)
10. Masindi (Myeeba VT 10,000m3) and
11. Lyantonde (Kanyogoga VT 10,000m3).
12. Butambala (Katabira VT 10,000m3),
13. Isingiro (Ntenga VT 20,000m3)
14. Sembabule (Lwera VT 20,000m3)
15. Kakumiro (Rwamadongo VT 20,000m3)